# Electric heater

The electric heater has a range of 0º C to 500º C. Use the slider to turn on the heater and adjust the temperature.

When heating a liquid, the rate at which the temperature rises is increased 20 or 30 times. This rapidly brings liquids to boiling point.

Tips for use:

- The temperature displayed on the front of the heater is usually not the same as the temperature of the contents of the vessel placed on it.

## See also:

- Bunsen burner
- Using chemistry parts