# Pictorial electronics parts

Pictorial parts are real-life representations of electronic components. They can be used to create simple circuits.

The following table lists additional key features of certain pictorial parts:

Part | Notes
--- | ---
Battery | Voltage: 1.5 V
1A Fuse | Current rating: 1 A (The part will explode once this 1 A current rating is exceeded.)
SPDT and SPDT switch | These are latching switches (the switch remains in the new state after being pressed). Each is operated by clicking on the switch button.
Push-to-make switch | On resistance: 0 ohms
Variable resistor | The resistance of the variable resistor can be varied from 0 to 500 ohms using the slider.
Resistor | Resistance: 680 ohms
Filament lamp | Maximum brightness voltage: 3.5 V Nominal voltage: 3.5 V
LED | Maximum brightness current: 10 mA Forward voltage at 10 mA: 1.9 V
Motor | Nominal voltage: 6 V Turn-on voltage: 0.7 V Explodes at maximum voltage: 12 V
Buzzer | Nominal voltage: 6 V Operate voltage: 3 V Resistance: 240 ohms

Tips for use:

- Pictorial parts can be wired like other electronic parts.
- Pictorial components are indestructible unless marked otherwise.

## See also

- Using electronics parts