# Signal lamp

The signal lamp has a linear current-voltage characteristic. The current is proportional to the applied voltage.

Part parameters:

- Nominal voltage: 6 V
- Maximum brightness at: 6 V
- Current at 6 V: 60 mA
- Maximum voltage: 9 V

Tips for use:

- Associate the Light intensity property of this part to the Incident light intensity property of an LDR to create a dependency.

## See also:

- Filament lamp
- LDR
- Using electronics parts