# Latching switch

A latching switch remains in the new state after being pressed. Click on the Switch button to operate it.

Types of latching switches:

- SPST (Single Pole Single Throw)
- SPDT (Single Pole Double Throw)
- DPST (Double Pole Single Throw)
- DPDT (Double Pole Double Throw)

Part parameters:

- On resistance: 0 ohms
- Maximum current: 15 A
- Maximum voltage: 400 V

## See also:

- Non-latching switch
- Using electronics parts