# Schmitt inverter

The Schmitt inverter part behaves in the same way as a standard Inverter part, but it has different threshold levels depending on whether the input is rising or falling. Above the threshold level the input voltage is recognised as binary '1'; below the threshold level it is recognised as binary '0'.

Truth table:

Input 1 | Output
--- | ---
0 | 1
1 | 0

Tips for use:

- The Schmitt inverter part is useful for interfacing logic to analogue signals.

## See also:

- Logic family parts
- Simulation of Digital ICs
- Using electronics parts