# Thermistor

Use the thermometer-slider to control the temperature of the thermistor. The temperature ranges from -20° C to +40° C in steps of 1° C, from the bottom to the top of the thermometer. As the temperature increases, the resistance of the thermistor decreases.

Click on the thermistor's resistance to edit it.

Part parameters:

- Maximum power dissipation: 250 W

## See also:

- Thermistor resistance variation
- Using electronics parts