# N-channel MOSFET

Tips for use:

- The substrate terminal of the MOSFET is not shown on the part. It is assumed that the substrate is connected to the source.

Part parameters:

- Gate threshold voltage: 1 V
- MOSFET constant: 1 A/V2
- Maximum gate-source voltage: 20 V
- Maximum gate-drain voltage: 20 V
- Maximum drain-source voltage: 400 V
- Maximum drain-source current: 20 A

## See also:

- Using electronics parts