# Transistor

The transistor is modelled as a silicon transistor.

Tips for use:

- Transistors can be flipped.

Part parameters:

- Temperature: 25° C
- Reverse current gain: 5
- Base ohmic resistance: 0 ohms
- Maximum current: 2 A
- Maximum power dissipation: 1 W
- Maximum collector-emitter voltage: 60 V
- Maximum collector-base voltage: 75 V
- Maximum emitter-base voltage: 5 V

## See also:

- Flipping parts
- Using electronics parts