# Latching digital inputs

Latching inputs remain in the new state after being pressed.

A Latching input part may have its own real-life context image. For example, a moisture sensor may show rain clouds; clicking the image causes the voltage amplitude to alternate between logic = 0 (no rain) and logic = 1 (rain).

## See also:

- Input and output power supplies
- Non-latching digital inputs
- Slider digital inputs
- Using electronics parts