# Operational amplifier

Tips for use:

- The operational amplifier can be flipped.
- The negative supply option is not available when simulating the 324 type op-amp.

Part parameters:

| 324 | 741
--- | --- | ---
Voltage gain | 100 000 (100 dB) | 20 000 (86 dB)
Unity gain bandwidth | 1 MHz | 1 MHz
Maximum slew rate | 0.5 V/µs | 0.5 V/µs
Maximum supply voltage | 32 V | ±36 V
Minimum total supply voltage | 3 V | 6 V
Output voltage swing (with 15 V supply) | 0 - 13.5 V | ±13 V
Output resistance | 75 ohms | 75 ohms
Short-circuit output current | 20 mA | 20 mA
Maximum input voltage (with 15 V supply) | -0.3 - 15 V | ±16 V

## See also:

- Flipping parts
- Using electronics parts