<< Previous | 1 | 2 | 3 | 4 | 5 | 6 | 7 | 8 | 9 | Next >>
Quickstart: Converting from Crocodile Technology
| real-PCB 2.0 can automatically generate PCB designs from circuit diagrams produced in Crocodile Technology 606 or later. Once you have completed your circuit diagram in a Crocodile Technology PCB space, click on the 'Export to real-PCB' button on the PCB space toolbar. This will start the conversion process. The conversion process will then guide you through all the steps required to turn your circuit diagram into a PCB layout. The Quick option will run the conversion with the default settings. The Custom option will allow you to customise these settings, with choices relating to board size, auto-placing, auto-routing and copper areas. With either of these options, when the conversion process is finished, your PCB design will then be automatically generated and displayed in Crocodile Technology according to the options you have chosen. The Manual conversion option is for advanced users and is similar to using real-PCB as a standalone application.
<< Previous Next >>