# Measuring current with the multimeter

Steps:

1. To measure current, there must be an ammeter in your 2D circuit. This will be represented by a terminal block in the 3D circuit.
2. Add the multimeter to the 3D space.
3. Set the dial to the appropriate current range.
4. Connect the multimeter probes to the terminal block to measure the current.
5. The measurement will be displayed on the multimeter screen.

## See also:

- Measuring voltage with the multimeter
- Multimeter
- Ammeter