# PIC programmer systems

The following PIC systems are supported by Crocodile Technology:

- Chip Factory (Pro), Revolution PIC Programmer: http://www.rev-ed.co.uk
- PICLab: http://www.madlab.org
- PICtalk: http://www.tep.org.uk

These systems are PIC Programmer systems, where the microcontroller is placed in the programmer for programming, and then placed into the target system once programmed. The PIC programmer is connected to the computer's serial (COM) port.

Crocodile Technology only supports direct programming of FLASH based microcontrollers (microcontrollers that can be reprogrammed a number of times). It does not support direct programming of OTP (one time programming) microcontrollers, although exported assembler code listings could be modified for these parts. When using the PIC programming systems it is important to select the correct microcontroller device. Attempted use of alternative microcontroller devices may cause unexpected results.

## See also:

- Plug-in software
- PIC programmers