# Burette

The burette is designed to dispense liquids accurately and is particularly useful for carrying out titrations. It has a fixed volume of 50 ml, measured to the nearest 0.01 ml.

Use the slider next to the burette to control the flow of liquid. The flow rate ranges from 0 (off) to 1 (fully on). You may also release the liquid one drop at a time by setting the flow rate to 0 (off) and then pressing the Add drop button once for each drop of liquid you wish to add.

The volume of liquid in the burette is always displayed.

## See also:

- Glassware
- Glassware toolbars
- Pasteur pipette
- Pipette